* Card reader makes cards use one subcarrier and high data rate
  + subcarrier frequency is fc/32 = 423.75 kHz